Configurar lan

|  |  |  |
| --- | --- | --- |
|  |  | Carrillos team  La Condamine N16-37  22504463 | info@carrillosteam.com | www.carrillosteam.com |

|  |  |  |
| --- | --- | --- |
| Red de Area Local  “Restart All Services” of WAMP and access your machine in **LAN**.  Bind the server static IP to the port number so for this you have be on the same file and change “**Listen 8081**”  to **“Listen 192.168.1.154:8081”**.  Make the WMAP Server accessible in the **LAN**, you have to get \wamp \ bin\ apache\ Apache2.2.11\ conf\ httpd.conf and open it and find the following code: |  | **Accesar WAMPSERVER desde una red de area local** To run the WAMP Apache server on your specified port, do the following. Go in the\wamp\bin\apache\Apache2.2.11\conf\httpd.conf file and search for **“#Listen”** and then change the port from 80 to 8081 and in that case, your URL will be **http://localhost:8081/**. Like below:  Listen 192.168.1.154:8081  <Directory "cgi-bin">  AllowOverride None  Options None  Order allow,deny  Allow from all  </Directory>  **open port**(8081) of the server such that everyone can access your server.  **Control Panel** >> **System and Security** >> **Windows Firewall** click on **“Advance Setting”**  select **“Inbound Rules”** click on **“Add Rule**”  Select **“PORT”** from the list and select **“TCP”** and enter port **“8081”** under **“Specific local port”** click on **”Next”** and select **“Allow the Connection”** and give name and description and click Done. |